**Web SBC set up lab for automation testing**

* Load all base configuration to testing lab (in /Data/Load\_Configuration)
  + Edit to your Lab IP using command:
    - sed –i ‘s/192.168.33.105/<your ip lab>/g’ <directory>/\*.cfg
* Edit to your lab IP in TPIP (BGCF, IBCF, PCSCF) and DNS (ICSCF, SCSCF) data excel files.
* Edit to your lab IP in InputData.robot in /Data (below is the IPs of web remote server and core SBC)
  + ${IP\_WEB\_SBC} = 192.168.33.110
  + ${BASE\_URL} = https://192.168.33.110
  + ${HOST\_SBC} = 192.168.33.105